# gsw_CT_from_entropy

    Conservative Temperature as a function of entropy

## Contents

- USAGE:
- DESCRIPTION:
- INPUT:
- OUTPUT:
- EXAMPLE:
- AUTHOR:
- VERSION NUMBER:
- REFERENCES:

## USAGE:

    CT = gsw_CT_from_entropy(SA,entropy)

## DESCRIPTION:

    Calculates Conservative Temperature with entropy as an input variable.

    Click for a more detailed description of calculating
    Conservative Temperature from entropy.

## INPUT:

    SA       =   Absolute Salinity                                  [ g/kg ]
    entropy  =   specific entropy                                  [ deg C ]

    SA & entropy need to have the same dimensions.

## OUTPUT:

    CT   =  Conservative Temperature                               [ deg C ]

## EXAMPLE:

    SA = [34.7118; 34.8915; 35.0256; 34.8472; 34.7366; 34.7324;]
    CT = [28.8099; 28.4392; 22.7862; 10.2262;  6.8272;  4.3236;]
    entropy = [400.3892; 395.4378; 319.8668; 146.7910; 98.6471; 62.7919;]

    CT = gsw_CT_from_entropy(SA,entropy)

    CT =

      28.8099
      28.4392
      22.7862
      10.2262
       6.8272
       4.3236

## AUTHOR:

    Trevor McDougall and Paul Barker [ help_gsw@csiro.au ]

## VERSION NUMBER:

    2.0 (13th October, 2010)

## REFERENCES:

    IOC, SCOR and IAPSO, 2010: The international thermodynamic equation of
     seawater - 2010: Calculation and use of thermodynamic properties.
     Intergovernmental Oceanographic Commission, Manuals and Guides No. 56,
     UNESCO (English), 196 pp.  Available from the TEOS-10 web site.
      See appendix  A.10 of this TEOS-10 Manual.

    The software is available from http://www.TEOS-10.org