# gsw_SonCl

    SP to Chlorinity ratio

## Contents

- USAGE:
- DESCRIPTION:
- OUTPUT:
- EXAMPLE:
- AUTHOR:
- VERSION NUMBER:
- REFERENCE:

## USAGE:

    SonCl = gsw_SonCl

## DESCRIPTION:

    The ratio of Practical Salinity, SP, to Chlorinity, 1.80655 kg/g for
    Reference Seawater (Millero et al., 2008).  This is the ratio that was
    used by the JPOTS committee in their construction of the 1978 Practical
    Salinity Scale (PSS-78) to convert between the laboratory measurements
    of seawater samples (which were measured in Chlorinity) to Practical
    Salinity.

## OUTPUT:

    SonCl  =  SP to Chlorinity ratio                           [ (g/kg)^-1 ]

## EXAMPLE:

    SonCl = gsw_SonCl

    SonCl =

      1.80655

## AUTHOR:

    Trevor McDougall and Paul Barker         [ help@teos-10.org ]

## VERSION NUMBER:

    3.01 (18th May, 2011)

## REFERENCE:

    Millero, F. J., R. Feistel, D. G. Wright, and T. J. McDougall, 2008:
      The composition of Standard Seawater and the definition of the
      Reference-Composition Salinity Scale, Deep-Sea Res. I, 55, 50-72.
       See section 5 below Eqn. (5.5) of this paper.

    The software is available from http://www.TEOS-10.org