# gsw_CT_from_pt

    Conservative Temperature from potential temperature

## Contents

- USAGE:
- DESCRIPTION:
- INPUT:
- OUTPUT:
- EXAMPLE:
- AUTHOR:
- VERSION NUMBER:
- REFERENCES:

## USAGE:

    CT = gsw_CT_from_pt(SA,pt)

## DESCRIPTION:

    Calculates Conservative Temperature of seawater from potential
    temperature (whose reference sea pressure is zero dbar).

    Click for a more detailed description of calculating
    Conservative Temperature from potential temperature.

## INPUT:

    SA  =  Absolute Salinity                                        [ g/kg ]
    pt  =  potential temperature (ITS-90)                          [ deg C ]

    SA & pt need to have the same dimensions.

## OUTPUT:

    CT  =  Conservative Temperature                                [ deg C ]

## EXAMPLE:

    SA = [34.7118; 34.8915; 35.0256; 34.8472; 34.7366; 34.7324;]
    pt = [28.7832; 28.4209; 22.7850; 10.2305;  6.8292;  4.3245;]

    CT = gsw_CT_from_pt(SA,pt)

    CT =

      28.809923015982083
      28.439144260767169
      22.786246608464264
      10.226165605435785
       6.827183417643142
       4.323565182322069

## AUTHOR:

    David Jackett, Trevor McDougall and Paul Barker  [ help@teos-10.org ]

## VERSION NUMBER:

    3.01 (5th May, 2011)

## REFERENCES:

    IOC, SCOR and IAPSO, 2010: The international thermodynamic equation of
     seawater - 2010: Calculation and use of thermodynamic properties.
     Intergovernmental Oceanographic Commission, Manuals and Guides No. 56,
     UNESCO (English), 196 pp.  Available from the TEOS-10 web site.
      See section 3.3 of this TEOS-10 Manual.

    The software is available from http://www.TEOS-10.org