# gsw_f

    Coriolis parameter (f)

## Contents

- USAGE:
- DESCRIPTION:
- INPUT:
- OUTPUT:
- EXAMPLE:
- AUTHOR:
- VERSION NUMBER:
- REFERENCE:

## USAGE:

    f = gsw_f(lat)

## DESCRIPTION:

    Calculates the Coriolis parameter (f) defined by:
         f = 2*omega*sin(lat)
    where,
         omega = 7.292115e-5   (Groten, 2004)                  [ radians/s ]

    Click for a more detailed description of the
    Coriolis parameter.

## INPUT:

    lat  =  latitude in decimal degrees north                [ -90 ... +90 ]

## OUTPUT:

    f    =  Coriolis parameter                                 [ radians/s ]

## EXAMPLE:

    lat = [ -90; -60; -30; 0;]

    f = gsw_f(lat)

    f =

    1.0e-003 *

      -0.145842300000000
      -0.126303136746351
      -0.072921150000000
                       0

## AUTHOR:

    20th April 1993. Phil Morgan          [ help@teos-10.org ]

    MODIFIED:
    28th July, 2010 by Paul Barker

## VERSION NUMBER:

    3.02 (17th November, 2012)

## REFERENCE:

    Groten, E., 2004: Fundamental Parameters and Current (2004) Best
      Estimates of the Parameters of Common Relevance to Astronomy, Geodesy,
      and Geodynamics. Journal of Geodesy, 77, pp. 724-797.

    IOC, SCOR and IAPSO, 2010: The international thermodynamic equation of
      seawater - 2010: Calculation and use of thermodynamic properties.
      Intergovernmental Oceanographic Commission, Manuals and Guides No. 56,
      UNESCO (English), 196 pp.  Available from the TEOS-10 web site.
       See appendix D of this TEOS-10 Manual.

    The software is available from http://www.TEOS-10.org