# gsw_C3515

    Conductivity of SSW at SP=35,t_68=15,p=0

## Contents

- USAGE:
- DESCRIPTION:
- OUTPUT:
- EXAMPLE:
- AUTHOR:
- VERSION NUMBER:
- REFERENCE:

## USAGE:

    C3515 = gsw_C3515

## DESCRIPTION:

    This function provides the present estimate of Conductivity, C, of
    Standard Seawater (SSW) at (SP=35, t_68=15, p=0) which is
    42.9140 mS/cm (=4.29140 S/m) (Culkin and Smith, 1980; UNESCO, 1983).

## OUTPUT:

    C3515  =  Conductivity at (SP=35, t_68=15, p=0)                [ mS/cm ]

## EXAMPLE:

    C3515 = gsw_C3515

    C3515 =

      42.9140

## AUTHOR:

    Trevor McDougall and Paul Barker          [ help@teos-10.org ]

## VERSION NUMBER:

    3.02 (17th November, 2012)

## REFERENCE:

    Culkin and Smith, 1980:  Determination of the Concentration of Potassium
      Chloride Solution Having the Same Electrical Conductivity, at 15C and
      Infinite Frequency, as Standard Seawater of Salinity 35.0000
      (Chlorinity 19.37394), IEEE J. Oceanic Eng, 5, 22-23.

    Unesco, 1983: Algorithms for computation of fundamental properties of
      seawater. Unesco Technical Papers in Marine Science, 44, 53 pp.

    The software is available from http://www.TEOS-10.org