# gsw_uPS

    unit conversion factor for salinities

## Contents

- USAGE:
- DESCRIPTION:
- OUTPUT:
- EXAMPLE:
- AUTHOR:
- VERSION NUMBER:
- REFERENCE:

## USAGE:

    uPS = gsw_uPS

## DESCRIPTION:

    The unit conversion factor for salinities (35.16504/35) g/kg (Millero et
    al., 2008).  Reference Salinity SR is uPS times Practical Salinity SP.

## OUTPUT:

    uPS  =  unit conversion factor for salinities                   [ g/kg ]

## EXAMPLE:

    uPS = gsw_uPS

    uPS =

      1.004715428571429

## AUTHOR:

    Trevor McDougall and Paul Barker          [ help@teos-10.org ]

## VERSION NUMBER:

    3.02 (17th November, 2012)

## REFERENCE:

    IOC, SCOR and IAPSO, 2010: The international thermodynamic equation of
      seawater - 2010: Calculation and use of thermodynamic properties.
      Intergovernmental Oceanographic Commission, Manuals and Guides No. 56,
      UNESCO (English), 196 pp.  Available from the TEOS-10 web site.
       See section 2.4 and Table D.4 of this TEOS-10 Manual.

    Millero, F. J., R. Feistel, D. G. Wright, and T. J. McDougall, 2008:
      The composition of Standard Seawater and the definition of the
      Reference-Composition Salinity Scale, Deep-Sea Res. I, 55, 50-72.
       See section 6, Eqn. (6.1) of this paper.

    The software is available from http://www.TEOS-10.org