# gsw_specvol

    specific volume (48-term equation)

## Contents

- USAGE:
- DESCRIPTION:
- INPUT:
- OUTPUT:
- EXAMPLE:
- AUTHOR:
- VERSION NUMBER:
- REFERENCES:

## USAGE:

    specvol = gsw_specvol(SA,CT,p)

## DESCRIPTION:

    Calculates specific volume from Absolute Salinity, Conservative
    Temperature and pressure, using the computationally-efficient 48-term
    expression for density (McDougall et al., 2013).

    Click for a more detailed description of specific volume.

## INPUT:

    SA  =  Absolute Salinity                                        [ g/kg ]
    CT  =  Conservative Temperature                                [ deg C ]
    p   =  sea pressure                                             [ dbar ]
           (ie. absolute pressure - 10.1325 dbar)

    SA & CT need to have the same dimensions.
    p may have dimensions 1x1 or Mx1 or 1xN or MxN, where SA and CT are MxN.

## OUTPUT:

    specvol  =  specific volume                                   [ kg/m^3 ]

## EXAMPLE:

    SA = [34.7118; 34.8915; 35.0256; 34.8472; 34.7366; 34.7324;]
    CT = [28.8099; 28.4392; 22.7862; 10.2262;  6.8272;  4.3236;]
    p =  [     10;      50;     125;     250;     600;    1000;]

    specvol = gsw_specvol(SA,CT,p)

    specvol =

     1.0e-003 *

       0.978626363206202
       0.978221861206179
       0.976154716658432
       0.972960929615236
       0.971026743358570
       0.968990291993136

## AUTHOR:

    Trevor McDougall and Paul Barker       [ help@teos-10.org ]

## VERSION NUMBER:

    3.02 (17th November, 2012)

## REFERENCES:

    IOC, SCOR and IAPSO, 2010: The international thermodynamic equation of
     seawater - 2010: Calculation and use of thermodynamic properties.
     Intergovernmental Oceanographic Commission, Manuals and Guides No. 56,
     UNESCO (English), 196 pp.  Available from the TEOS-10 web site.
      See Eqn. (2.7.2) of this TEOS-10 Manual.

    McDougall T.J., P.M. Barker, R. Feistel and D.R. Jackett, 2013:  A
     computationally efficient 48-term expression for the density of
     seawater in terms of Conservative Temperature, and related properties
     of seawater.  To be submitted to J. Atm. Ocean. Technol., xx, yyy-zzz.

    The software is available from http://www.TEOS-10.org