# gsw_cp0

    the "specific heat" for use with
    Conservative Temperature

## Contents

- USAGE:
- DESCRIPTION:
- OUTPUT:
- EXAMPLE:
- AUTHOR:
- VERSION NUMBER:
- REFERENCE:

## USAGE:

    cp0 = gsw_cp0

## DESCRIPTION:

    The "specific heat" for use with Conservative Temperature.  cp0 is the
    ratio of potential enthalpy to Conservative Temperature.

## OUTPUT:

    cp0  =  The "specific heat" for use                         [ J/(kg K) ]
            with Conservative Temperature

## EXAMPLE:

    cp0 = gsw_cp0

    cp0 =

      3991.86795711963

## AUTHOR:

    Trevor McDougall and Paul Barker          [ help@teos-10.org ]

## VERSION NUMBER:

    3.02 (17th November, 2012)

## REFERENCE:

    IOC, SCOR and IAPSO, 2010: The international thermodynamic equation of
      seawater - 2010: Calculation and use of thermodynamic properties.
      Intergovernmental Oceanographic Commission, Manuals and Guides No. 56,
      UNESCO (English), 196 pp.  Available from the TEOS-10 web site.
       See Eqn. (3.3.3) and Table D.5 of this TEOS-10 Manual.

    The software is available from http://www.TEOS-10.org